EXPERIMENT 25

Write an assembly language program to swap two 8-bit datausing 8085 processor.

CODE:

LDA 2500

MOV B,A

LDA 2501


STA 2500

MOV A,B

STA 2501

HLT

OUTPUT:



RESULT:

