EXPERIMENT 3

Write an assembly language program for adding two 16-bit datausing 8086 processor

CODE:

LDA 8500

MOV B,A

LDA 8501

MOV C,A

LDA 8502

MOV D,A

LDA 8503

ADD C


STA 8505

MOV A,D

ADD B

STA 8504

RST 1

.