EXPERIMENT 5

Write an assembly language program for multiplication of two 8-bit data A7 A6 A5 A4 A3 A2 A1 A0 and B7 B6 B5 B4 B3 B2 B1 B0 using 8085 processor.

CODE:

LDA 8500

MOV B,A

LDA 8501

MOV C,A

CPI 00

JZ LOOP

XRA A

LOOP1: ADD B

DCR C

JZ LOOP

JMP LOOP1

LOOP: STA 8502

HLT

